		
			    Kill Gle 16

These examples are too large for the normal 16-Bit DOS-Versions MANIP and
( C, HP, PS, DVI, ...)GLE. GLE32 has absolutely no problems.

Axel Rohde

P.S.: You can see the phase relation between the response and the sinusoidal
      driver of a driven Van der Pol oscillator: a) Adlers Equation
      b) numerical results.
      You can see the periodicly incomplete phase-locking. In the frequency
      domain, this behavior produces a single-sided triangular spectrum
      due to simultaneous amplitude- and frequency modulation.
      The phenomenon is known as 'periodic pulling'. The oscillators
      frequency is pulled periodicly to the driver frequency.
