			    CM11.OCX


			Short description



Object CM11 from CM11.OCX has next possibilities :

Communication through X-10

Properties :
	
	Init		- serial port for CM11 
			   After seting this properties will be execution initialization interface CM11
	Address		- Address of X-10 element  ("A4" …)  		As String
	Value		- value for Preset Dim				As Integer	
	Command	- Command from next List  (for this moment)	As String
				"ON"		= On
"OFF"		= Off
"ALLON"	= All Lights On
"ALLUOFF"	= All Units Off
"ALLOFF"	= All Lights Off
"DIM"		= Dim
"BRG"		= Bright
"DNL"		= Download all bytes from Address to CM 11 memory
		    from address 0
"SETTIME"	= Current Time from Computer is send to CM11
"GETTIME"	= Request to CM11 for Read set Time 
		    Result is  String after InputX10 Event
		    Time in format interface CM11 it means 14 bytes

	After seting this properties will be Command performed

      Example :
	
CM111.Address = "A3"
CM111.Value = 0
CM111.Command = "ON"

Event :

	X10Input (Buffer As String)
		After receive  command from X-10 string contens :
			"A 2"	= selected element A2
			"AON"	= Command "ON" for House Code "A"


	Result (Code As Integer)

	Code = 0 - Command performed OK
	             1 - Command not performed
	             9 - Init command can not open defined port
 	             8 -  After "Init" - communication with interface CM11 not O.K.
